Mobo notes:

* Board thickness – 1mm
* Bottom screen connector thickness (including board) – 3mm
* Cart slot height – 7mm (not including board)